void setup(){

pinMode(9, OUTPUT);

pinMode(2, INPUT);

}

void loop() {

if(digitalRead(2) == LOW){

digitalWrite(9, HIGH);

delay(1000);

//turn the LED ON by making voltage HIGH

// wait 1 second

}

else{

digitalWrite(9, LOW); delay(1000); //turn the LED OFF by making voltage LOW

}